**Røde Wireless GO II**

Operating Instructions

Full details: <https://rode.com/wirelessgoii/learning-hub>

Quick Set-Up:

* Plug Receiver into Laptop
* Turn Transmitter and Receiver “On”
* Select “WIRELESS GOTO II RX” when setting up audio. If using a webcam, be sure to disable that mic to avoid echo or feedback.
* Attach transmitter somewhere close to the centerline of the body (to cut down on doppler effect when rotating the head)

When using with Webcam:

* Plug Webcam into laptop
* Position Webcam (either on stand or on screen)
* In “Video Settings” choose “C922 Pro Stream Camera”



A picture containing text

Description automatically generated



Background pattern

Description automatically generated with low confidence

 **Connecting to Computers**

Use the supplied USB-C to USB-A cable to connect the Wireless GO II receiver to any computer with a USB-A input (use USB-C to USB-C cable for computers with a USB-C input), then go to your audio settings and select ‘Wireless GO II RX’ as your input device. This essentially turns the Wireless GO II receiver into a wireless USB audio interface.